;/*++
;
;Module Name:
;
;    SLABVCP.INF
;
;    Copyright 2012, Silicon Laboratories
;
;Abstract:
;    Installation INF for Silicon Laboratories CP210x device using KDMF Version 1.9
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Provider%
DriverVer=12/10/2012,6.6.1.0
CatalogFile=slabvcp.cat


; ================= Device section =====================

[Manufacturer]
%MfgName%=SiLabs, NTamd64

[SiLabs]
%USB\VID_10C4&PID_EA60.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA60
%USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA70&Mi_00
%USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA70&Mi_01
%USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_00
%USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_01
%USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_02
%USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_03

[SiLabs.NTamd64]
%USB\VID_10C4&PID_EA60.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA60
%USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA70&Mi_00
%USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA70&Mi_01
%USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_00
%USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_01
%USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_02
%USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc%=silabser.Dev, USB\VID_10C4&PID_EA71&Mi_03

[silabser.Dev.NT]
Include=msports.inf
AddReg=silabser.AddReg,silabser.NT.AddReg
CopyFiles=silabser.Files.Ext

[silabser.Dev.NT.Services]
Include=msports.inf
Addservice = silabenm,,silabenm.AddService
Addservice = silabser,0x00000002,silabser.AddService

[silabser.AddService]
DisplayName    = %silabser.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\silabser.sys
LoadOrderGroup = Extended Base

[silabenm.AddService]
DisplayName    = %silabenm.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\silabenm.sys
LoadOrderGroup = PNP Filter

; common registry entries 
[silabser.AddReg]
HKR,,NTMPDriver,,silabser.sys
HKR,,RateLimitPurgeMS, 0x10001, 0x64, 0x00, 0x00, 0x00
HKR,,OverrideDefaultPortSettings, 0x10001, 01,00,00,00
HKR,,InitialBaudRate, 0x10001, 00,C2,01,00		;115200 initial baud rate
HKR,,InitialLineControl,, "8N1"				;8-bits, No parity, 1 stop bit

[silabser.NT.AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[silabser.Dev.NT.HW]
AddReg=silabser.Dev.NT.HW.AddReg

[silabser.Dev.NT.HW.AddReg]
HKR,,"UpperFilters",0x00010008,"silabenm"
HKR,,"SelectiveSuspendTimeout",0x00010001,10000

[silabser.Files.Ext]
silabser.sys
silabenm.sys

[SourceDisksNames.x86]
1=%Disk_Description%,"silabser.sys",,\x86

[SourceDisksNames.amd64]
1=%Disk_Description%,"silabser.sys",,\x64

[SourceDisksFiles]
silabser.sys = 1
silabenm.sys = 1

[DestinationDirs]
Silabser.Files.Ext = 12

;-------------- WDF Coinstaller installation

[DestinationDirs]
CoInstaller_CopyFiles = 11

[silabser.Dev.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoinstaller01009.dll

[SourceDisksFiles]
WdfCoinstaller01009.dll=1

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoinstaller01009.dll,WdfCoInstaller"

[silabser.Dev.NT.Wdf]
KmdfService = silabser, silabser_wdfsect
[silabser_wdfsect]
KmdfLibraryVersion = 1.9

;---------------------------------------------------------------;

[Strings]
Provider="Silicon Laboratories"
MfgName="Silicon Laboratories"
Disk_Description="Silicon Labs USB to UART Bridge Installation Disk"
USB\VID_10C4&PID_EA60.DeviceDesc="Silicon Labs CP210x USB to UART Bridge"
USB\VID_10C4&PID_EA70&Mi_00.DeviceDesc="Silicon Labs Dual CP210x USB to UART Bridge: Enhanced COM Port"
USB\VID_10C4&PID_EA70&Mi_01.DeviceDesc="Silicon Labs Dual CP210x USB to UART Bridge: Standard COM Port"
USB\VID_10C4&PID_EA71&Mi_00.DeviceDesc="Silicon Labs Quad CP210x USB to UART Bridge: Interface 0"
USB\VID_10C4&PID_EA71&Mi_01.DeviceDesc="Silicon Labs Quad CP210x USB to UART Bridge: Interface 1"
USB\VID_10C4&PID_EA71&Mi_02.DeviceDesc="Silicon Labs Quad CP210x USB to UART Bridge: Interface 2"
USB\VID_10C4&PID_EA71&Mi_03.DeviceDesc="Silicon Labs Quad CP210x USB to UART Bridge: Interface 3"
silabser.SvcDesc="Silicon Labs CP210x USB to UART Bridge Driver"
silabenm.SvcDesc="Silicon Labs CP210x USB to UART Bridge Serial Port Enumerator Driver"
PortsClassName = "Ports (COM & LPT)"
